*Translation from Latvian*

**Annex No. 1.**

**Specification for a lorry trailer (residential caravan)**

Residential caravan mounted on the frame of the two-axle lorry trailer. Trailer with the caravan has been registered with the Road Traffic Safety Directorate (CSDD):

* category – “O”, depending on weight,
* type – “Residential lorry trailer”,
* registration No., permitting participation in road traffic without restrictions,
* length: 7.5-8.0 metres,
* galvanised trailer frame,
* front axle of the trailer – turnable with a fixation option,
* desirable distance from the lowest point of the trailer and the footprint (clearance) – 500 mm.

|  |  |
| --- | --- |
| **Item No. in the drawing** | **Name of the item reflected in the drawing** |
| 1 | Double bunk bed. |
| 2 | Foldable table. |
| 3 | Cabinet. |
| 4 | Sliding door. |
| 5 | Changing room.  |
| 6; 7; 8; 9 | Refrigerator/cabinet with a table/electric cooker/sink. |
| 10 | Water reservoir (100-150 litres). |
| **Equipment that is not shown in the sketch** |
| Heat penetration coefficient of external walls and floor: U ≤ 0.54 [W/(m2K)]\*. |
| All electrical equipment – for 220V voltage with cables cased over the plaster. Insulation resistance measurements of the wiring are preferable. |
| Electrical heating (3 oil radiators 1.5-2.0 kW with a regulator). |
| Electrical sockets over the plaster in the casing for wiring (at least 8 pcs). Placement and number shall be agreed upon during the process of manufacture. |
| External lighting of the entrance door and stairs that can be switched on from indoors. |
| Voltage distribution cabinet (for various consumers). |
| Forced ventilation above the cooker and natural ventilation in rooms. |
| Ventilation openings to ensure air exchange in the sleeping room |
| 3-5 windows (1-2 of those can be opened (with a mosquito net) to ensure exchange of air in the rooms). Placement shall be agreed upon during the process of manufacture. |
| A place and fastening for 2 fire extinguishers with the extinguishing capacity of 27A144B. |
| Fire alarms in the sleeping room and common room.  |
| Air-tight box for transportation of diesel generator and other equipment. Sizes and placement shall be agreed upon during the process of manufacture. |
| Air-tight cabinet with sockets for connection of electricity supply from a 3-phase generator or network with the voltage of ~ 230/400 V. |
| Water supply circuit for the kitchen sink. Water reservoir with swing blocking partition walls and a hatch for washing.  |
| Mandatory option to empty the water supply circuit to prevent the freezing of the system when ambient air temperature is below 0 degrees C. |
| Foldable stairs at the entrance door. Retractable waterproof sun-blind above the entrance door. |

Dimensions of the caravan; internal placement of doors, windows and equipment in the sketch is of recommendation nature. Proposals and technical solutions submitted by the tenderers shall be reviewed.

To be provided in the tender:

1. Model of the separate assemblage items (cooker, refrigerator, etc.), costs, and a model for alternative solutions with costs;
2. The required advance payment and interim payments during the production process;
3. Delivery (production and commissioning pursuant to specification) period from the moment of signing the contract.